**TENDER NOTICE**

**TENDER NO. RGM-NTR-I/Prj-1836/Civil-Work/Open-Surface-Drain/2019-20/03/**

**TENDER FOR WATER LINE & BATHROOM WORKS AT CITY COLONY KHYBER BAZAR PESHAWAR**

Sealed bids are invited for **Tender for CIVIL WORKS WATER LINE & BATHROOM WORKS at City Colony Khyber Bazar Peshawar** In accordance with Technical Specifications, Scope of Work and BOQ as specified in the Tender documents.

* Bids shall be submitted in Room #:217, Telephone Office, 1 The Mall Peshawar Cantt as per instructions provided in tender documents on or before 12:00 Hr. Dated: **13-09-2019**.
* Tender documents can be purchased from the undersigned on payment of Rs. 1000/.- (non-refundable) through Demand Draft/pay order in favor of Senior Manager (Finance) NTR-1, Peshawar.
* Bids received after the above deadline shall not be accepted and be returned unopened. Bids through E-mail / Fax / Courier shall not be accepted.
* Commercial bids must be accompanied by a bid security of 2% of the total cost. **In case of non-compliance, the bids will be disqualified from further processing.**
* PTCL reserves the right to reject any or all bids and to annul the bidding process at any time, without thereby incurring any liability to the affected bidder (s) or any obligation to inform the affected bidder (s) of the grounds for PTCL action.
* Only Medium / Large Category PTCL registered vendors are invited to participate. However, bids from willing reputed vendors (Un-registered vendor) with experience of 5-10 years regarding scope of work may be entertained with the condition that they will comply with PTCL standards and get themselves registered. In case vendor is not registered, then registration must be done before the issuance of Letter of Intent/Award (LOI/LOA).
* Bidders must submit their bids (including GST) with given format and complete in all respect. Incomplete/partial bids will not be entertained and the bidder will be disqualified without any further notice. Bidders shall ensure that all RFP clauses and their compliance are filled adequately. RFP compliance once submitted by bidders (duly filled and signed) shall remain valid till signing of the contract.
* PAYMENTS AND PENALTIES
* Running payment schedule would be as follows: -
* 50% Completion - 30% Payment
* 80% Completion - 20% Payment
* 100% Completion - 30% Payment
* On final verification 20 % Payment

Penalty: Penalty will be imposed as per JPM in case of delay completion of the work.

* Bidder must mention their Vendor Registration code on quotation. In case vendor is not registered, then registration must be done before the issuance of Letter of Intent (LOI). Vendor Registration form can be downloaded from PTCL website [www.ptcl.com.pk/media](http://www.ptcl.com.pk/media).
* **Rates may clearly be mentioned on % below, above or at par on the basis of MES schedule of rates 2014 where applicable.**
* All correspondence on the subject may be addressed to the undersigned.

**Ibrar Hussain**

**SM (Regional Procurement)**

**Telephone House, Room No:119**

**1 The Mall, Peshawar Cantt**

**Tel: +92-91-5276013**

**Email:** **Ibrar.Hussain1@ptcl.net.pk**

|  |
| --- |
| **RFQ for Water line & Bathroom work at City Colony Khyber Bazar Peshawar** |
| **Sl #** | **Page &Item #** | **Description** | **Qty** | **Unit** | **Rate** | **Amount** |
|
|  |  | **Bath Room internal fitting & Accessories** |  |  |  |  |
| **1** |  | **Demolition of Concrete**  |  |  |  |  |
|  | **23-1** | Demolition of **un-reinforced or CC** and etc. |  |  |  |  |
|  |  | **Block-1** |  |  |  |  |
|  |  | **Total F P S**  | **1,757.25** | **Cft** |  |  |
|  |  | **Total M K S**  | **49.77** |  **Cum** |  |  |
| **2** |  | **Disposal of Metrial/mulba etc** |  |  |  |  |
|  | **01-18+19+20** | Load “materials” (like demolished brick bats, bricks, sand and bitumen etc) on truck/ trolley or any other means, carry upto 100 M or part thereof, unload and stack or spread. |  |  |  |  |
|  |  | **Total F P S**  | **1,757.25** | **Cft** |  |  |
|  |  | **Total M K S**  | **49.77** |  **Cum** |  |  |
| **3** |  | **PVC 4" dia Class B ( Popular)** |  |  |  |  |
|  | **18-452** | Providing and fixing uPVC pipe 4" dia Class B including all fitting as required i/c dismantling of slabs or walls for hole and grouted with PCC 1:2:4. |  |  |  |  |
|  |  | **Total F P S**  | **1,491.00** | **Rft** |  |  |
|  |  | **Total M K S**  | **454.43** | **Mtr** |  |  |
| **4** |  | **PVC 3" dia Class B ( Popular)** |  |  |  |  |
|  | **18-451** | Providing and fixing uPVC pipe 3" dia Class B including all fitting as required i/c dismantling of slabs or walls for hole and grouted with PCC 1:2:4. |  |  |  |  |
|  |  | **Total F P S**  | **1,491.00** | **Rft** |  |  |
|  |  | **Total M K S**  | **454.43** | **Mtr** |  |  |
| **5** |  | **WC Asiatic (Porta make)** |  |  |  |  |
|  | **17-39** | Supply and fix, **Closet Pan only**, Asiatic pattern, **special colour.** full **Orrisa** pattern or equivalent, incl connection to trap and flushing pipe, incl making good to floor, best quality. |  |  |  |  |
|  |  | **Total M K S**  | **88.00** | **Nos** |  |  |
| **6** |  | **Flushing cistern glazed (Porta make )** |  |  |  |  |
|  | **17-41** | Supply and fix, **Low down cistern**, glazed, **white** colour, 13 lit capacity (incl brackets if required) and connection to flush pipe, best quality,  |  |  |  |  |
|  |  | **Total M K S**  | **88.00** | **Nos** |  |  |
| **7** |  | **Tee Stop Cock Master Make Code# 068** |  |  |  |  |
|  | **18-234** | Stop cock brass, CP, screw down, high pressure, fancy type, 15mm dia, supply and fixing. |  |  |  |  |
|  |  | Flushing cistern | **88.00** | **Nos** |  |  |
|  |  | **Total M K S**  | **88.00** | **Nos** |  |  |
| **8** |  | **Bib cock, Master Make Code# 068** |  |  |  |  |
|  | **18-215** | Bib cock, Brass, CP, fancy type, screwed down, BSP, 15 mm dia, supply and fixing. |  |  |  |  |
|  |  | Toilet | **88.00** | **Nos** |  |  |
|  |  | **Total M K S**  | **88.00** | **Nos** |  |  |
| **9** |  | **PCC 1:2:4** |  |  |  |  |
|  | **12-15** | Providing and laying CC Type ‘B’ as in floor, slabs, surface finished smooth with neat cement and steel trowel, using shingle or gravel. |  |  |  |  |
|  |  | **Total F P S**  | **2,746.25** | **Cft** |  |  |
|  |  | **Total M K S**  | **77.77** |  **Cum** |  |  |
| **10** |  | **Taking down Doors & windows** |  |  |  |  |
|  | **07-205** | Taking down partitions, framing, cupboard front, wall panelling and similar woodwork, incl doors exc 2.60m super each, Hard / Soft wood. |  |  |  |  |
|  |  | **Total F P S**  | **1,540.00** | **Sft** |  |  |
|  |  | **Total M K S**  | **143.12** | **Sqm** |  |  |
| **11** |  | **Steel Chowkat** |  |  |  |  |
|  | **07-228** | Supply & fix, Steel Chowkat press-moulded 16 SWG, for 115mm walls, single leaf, complete, incl hold fast ties for lateral movement, PCC 1:2:4 cavity filling etc, incl one coat of anti-Creosote paint (internal surface and Red oxide paint (external surface). |  |  |  |  |
|  |  | **Total F P S**  | **1,364.00** | **Rft** |  |  |
|  |  | **Total M K S**  | **415.73** | **Mtr** |  |  |
| **12** |  | **Door shutter** |  |  |  |  |
|  | **07-119** | Supply and fix, MDF (Medium Density Fibre board ) Hollow Flush door 38mm thick with Malaysian ply (Pak made) 3mm skin panel on both sides internal wood, 2nd class soft wood frame, 75mm x32mm, hydraulically hot pressed with glue, in any design, shape and pattern, complete, incl iron mongery, except chowkat. |  |  |  |  |
|  |  | **Total F P S**  | **1,430.00** | **Sft** |  |  |
|  |  | **Total M K S**  | **132.90** | **Sqm** |  |  |
| **13** |  | **Painting Steel work on chowkat** |  |  |  |  |
|  | **15-58** | 1st Coat of painting on new or old work such as steel doors, windows and CSWs of any type and description with **Synthetic Enamel paint**. |  |  |  |  |
|  | **15-59** | Same as item 15-58, but 2nd and subsequent coat. |  |  |  |  |
|  |   | **Total F P S**  | **520.52** | **Sft** |  |  |
|  |   | **Total M K S**  | **48.38** | **Sqm** |  |  |
| **14** |   | **Door shutter with chowkat Paint work** |  |  |  |  |
|  | 15-33 | **Prime Coat** on new wood work such as timber work in ceiling timber boarding etc., of any description, as specified. |  |  |  |  |
|  | 15-34 | Ist Coat of painting on new or old work such as timber work ceiling and timber boarding etc of any description with synthetic enamel paint. |  |  |  |  |
|  | 15-35 | Same as item 15-34, but second and subsequent coat. |  |  |  |  |
|  |  | **Total F P S**  | **2,860.00** | **Sft** |  |  |
|  |  | **Total M K S**  | **265.80** | **Sqm** |  |  |
| **15** |  | **Scraping plaster** |  |  |  |  |
|  | **13-19** | Hacking Cement Plaster of walls or lathing, racking out joints when required, or racking out cement jointing to walls, roofs or floors of any description, or hacking out concrete to form key, or dismantling, lathing with or without plaster |  |  |  |  |
|  |  | **Total F P S**  | **19,905.60** | **Sft** |  |  |
|  |  | **Total M K S**  | **1,849.23** | **Sqm** |  |  |
| **16** |  | **19mm Cement Palaster** |  |  |  |  |
|  | **13-13** | 19mm thick Cement Plaster 1:6, finished as specified |  |  |  |  |
|  |  | **Total F P S**  | **19,905.60** | **Sft** |  |  |
|  |  | **Total M K S**  | **1,849.23** | **Sqm** |  |  |
|  |  | **water supply line.** |  |  |  |  |
| **17** |  | **GI pipe (medium) ILL kirachi 1/2" dia** |  |  |  |  |
|  | **18-9** | **Tube, Water Quality (GI)** with all fittings (i.e sockets, bends, tees, elbows where required) and laid complete in trenches (excl excavation) or fixed to wall, floor (surface or concealed) and ceiling etc, incl caps and plugs as required 15mm dia **(medium),** supply and fixing. |  |  |  |  |
|  |  | **Total F P S**  | **2,720.00** | **Rft** |  |  |
|  |  | **Total M K S**  | **829.06** | **Mtr** |  |  |
| **18** |  | **GI pipe (medium) ILL kirachi 3/4" dia** |  |  |  |  |
|  | **18-10** | **Tube, Water Quality (GI)** with all fittings (i.e sockets, bends, tees, elbows where required) and laid complete in trenches (excl excavation) or fixed to wall, floor (surface or concealed) and ceiling etc, incl caps and plugs as required 20mm dia **(medium),** supply and fixing. |  |  |  |  |
|  |  | **Total F P S**  | **674.50** | **Rft** |  |  |
|  |  | **Total M K S**  | **205.59** | **Mtr** |  |  |
| **19** |  | **GI pipe (medium) ILL kirachi 1-1/2" dia** |  |  |  |  |
|  | **18-12** | **Tube, Water Quality (GI)** with all fittings (i.e sockets, bends, tees, elbows where required) and laid complete in trenches (excl excavation) or fixed to wall, floor (surface or concealed) and ceiling etc, incl caps and plugs as required 40mm dia **(medium),** supply and fixing. |  |  |  |  |
|  |  | **Total F P S**  | **800.00** | **Rft** |  |  |
|  |  | **Total M K S**  | **243.84** | **Mtr** |  |  |
| **20** |  | **PPR Pipe for ineternal bathroom fitting** |  |  |  |  |
|  | **18-894** | **PPR pipe, with all fittings i.e. socket, bend, tee, elbow, where required, 25 mm dia, Class PN-20 (excl excavation), supply and fixing.** |  |  |  |  |
|  |  | **Total F P S**  | **2000.00** | **Rft** |  |  |
|  |  | **Total M K S**  | **609.57** | **Mtr** |  |  |
| **21** |  | **Demolition of Concrete floor** |  |  |  |  |
|  | **23-1** | Demolition of **un-reinforced lime or CC** and **Premix carpet** etc. |  |  |  |  |
|  |  | **Total F P S**  | **287.50** | **Cft** |  |  |
|  |  | **Total M K S**  | **8.14** |  **Cum** |  |  |
| **22** |  | **Excavation** |  |  |  |  |
|  | **01-1** | **Excavation** as in **Ordinary Soil upto 1.5 M depth**, in foundation and pipe trenches upto 1.5 M wide, in shafts, wells and independent holes upto 30 sqm each and throw earth clear of edges of excavation within 10m. Timbering to be paid extra *(Foundation and Trench over 1.5 M widths will be treated as* ***Areas****)*.  |  |  |  |  |
|  |  | **Total F P S**  | **862.50** | **Cft** |  |  |
|  |  | **Total M K S**  | **24.43** |  **Cum** |  |  |
| **23** |  | **Disposal of Metrial/mulba etc** |  |  |  |  |
|  | **01-18+19+20** | Load “materials” (like demolished brick bats, bricks, sand and bitumen etc) on truck/ trolley or any other means, carry upto 100 M or part thereof, unload and stack or spread. |  |  |  |  |
|  |  | **Total F P S**  | **632.50** | **Cft** |  |  |
|  |  | **Total M K S**  | **17.91** |  **Cum** |  |  |
| **24** |  | **GI pipe (medium) ILL kirachi 3" dia** |  |  |  |  |
|  | **18-15** | **Tube, Water Quality (GI)** with all fittings (i.e sockets, bends, tees, elbows where required) and laid complete in trenches (excl excavation) or fixed to wall, floor (surface or concealed) and ceiling etc, incl caps and plugs as required 80mm dia **(medium),** supply and fixing. |  |  |  |  |
|  |  | **Total F P S**  | **362.00** | **Rft** |  |  |
|  |  | **Total M K S**  | **110.34** | **Mtr** |  |  |
| **25** |  | **GI pipe (medium) ILL kirachi 4" dia** |  |  |  |  |
|  | **18-16** | **Tube, Water Quality (GI)** with all fittings (i.e sockets, bends, tees, elbows where required) and laid complete in trenches (excl excavation) or fixed to wall, floor (surface or concealed) and ceiling etc, incl caps and plugs as required 100mm dia **(medium),** supply and fixing. |  |  |  |  |
|  |  | **Total F P S**  | **213.00** | **Rft** |  |  |
|  |  | **Total M K S**  | **64.92** | **Mtr** |  |  |
| **26** |  | **Sluice Valves 4" dia** |  |  |  |  |
|  | **18-263** | Sluice Valve, according to **BSS-5150/5163, PN-16 (Table18-1-7).** flanged and drilled to BS Table 18-1-9, complete with rubber packing, 80 mm dia, supply and fixing. |  |  |  |  |
|  |  | **Total F P S**  | **3.00** | **Nos** |  |  |
|  |  | **Total M K S**  | **3.00** | **Nos** |  |  |
| **27** |  | **PCC 1:4:8** |   |   |   |   |
|  | **12-3** | Providing and laying CC 1:4:8, laid under floor using shingle or gravel **Detail MES schedule Pakistan -2014 SECTION - 12.** |   |   |   |   |
|  |  | **Total F P S**  | **143.75** | **Cft** |  |  |
|  |  | **Total M K S**  | **4.07** | **Cum** |  |  |
| **28** |  | **PCC Type ‘B’ (1:2:4 ) floor** |  |  |  |   |
|  | **12-19** | Providing and laying, CC Type ‘B,’ using Crush , **Detail MES schedule Pakistan -2014 SECTION - 12** laid in floor, slabs as under layer for Terrazzo / Stonolithic / tiles top finished. |   |   |   |   |
|  |  | **Total F P S**  | **143.75** | **Cft** |  |  |
|  |  | **Total M K S**  | **4.07** | **Cum** |  |  |
| **29** |  | **Manholes, complete for**  |  |  |  |  |
|  | **21-25** | Manholes, complete, rectangular or circular as described, not exc 600mm deep from invert to surface of cover, incl main channel, set in CM 1:1,230 mm thick brick walls (Except Manhole cover). |  |  |  |  |
|  |  | **Total F P S**  | **24.00** | **Cft** |  |  |
|  |  | **Total M K S**  | **0.68** |  **Cum** |  |  |
| **30** |  | **Manholes Cover** |  |  |  |  |
|  | 21-35 | Providing and laying, RCC Type ’B’ manhole cover (Precast) complete with angle iron frame, embedded in concrete, all as per Information Sheet # Svcs-341 |  |  |  |  |
|  |  | **Total M K S**  | **3.00** | **Nos** |  |  |
|  |  | **T O T A L** |  |
|  |  | **(Below, Above, At par %age) on MES Schedule Rate 2014** |  |
|  |  | **Added 15% SST** |  |
|  |  | **Grand Total** |  |

|  |  |
| --- | --- |
| logo | **Pakistan Telecommunication Company Limited Office of the Regional General Manager, NTR-I, PTCL Peshawar** **Terms & condition** |

**RFQ No. . RGM NTR-I/RPC/2019/**

**RFQ for Water Line and Bathroom works at City Khyber Bazar colony Peshawar**

1. **Sealed bids, in Pak** Rupees on DDP basis, are invited for the **“Water Line and Bathroom works at city Khyber bazar colony** “.
2. Tender documents can be purchased from Manager Procurement NTR-1 up-to 29-08-2019 on payment of PKR 1500/- (non-refundable) through Demand Draft / Pay Order in favor Senior Manager (Finance) NTR-I, Peshawar.
3. Bids with bid security of Rs. 02% in shape of bank draft/CDR should be submitted / dropped in bid box as per instructions given to the bidders contained in the Bid Documents / RFP by 11:30 AM on 05-09-2019 positively. In case of non-compliance, bids will be disqualified for further processing. Bid(s) received after the above mentioned deadline shall not be accepted.
4. All bidders shall be called for presentations on MS Power Point to explain plan of execution of the anticipated awarded work to Technical Evaluation Committee.
5. PTCL reserves the right to reject any or all bids and to annul the bidding process at any time, without thereby incurring any liability to the affected bidder(s) or any obligations to inform the affected bidder(s) of the grounds for PTCL’s action.
6. Compliance of PTCL standard payments terms and delivery period, given in tender documents is mandatory for participation in bid. Successful bidder after award of work will ensure pictures are taken before execution, during execution and after completion of work.
7. Only Medium / Large Category PTCL registered vendors are invited to participate. However, bids from willing reputed vendors (Un-registered vendor) with experience of 5-10 years regarding scope of work may be entertained with the condition that they will comply with PTCL standards and get themselves registered. In case vendor is not registered, then registration must be done before the issuance of Letter of Intent/Award (LOI/LOA).
8. Bidders must submit their bids (including GST) with given format and complete in all respect. Incomplete/partial bids will not be entertained and the bidder will be disqualified without any further notice. Bidders shall ensure that all RFP clauses and their compliance are filled adequately. RFP compliance once submitted by bidders (duly filled and signed) shall remain valid till signing of the contract.

**PAYMENTS AND PENALTIES**

1. Running payment schedule would be as follows: -
2. 50% Completion - 30% Payment
3. 80% Completion - 20% Payment
4. 100% Completion - 30% Payment
5. On final verification 20% Payment

Penalty: Penalty will be imposed as per JPM in case of delay completion of the work.

1. All correspondence on the subject may be addressed to the undersigned

**SM Procurement**

Room no. 119,

Telephone House, 1-The Mall, Peshawar

Phone: